"X) Xmodem___________(Internal)
",0,IX,8,,,128,,0.78,,,,
"2) Xmodem___________(Qmxfer)
",0,S,8,,,128,,0.78,,,"C:QMXFER.COM -s -f [FILE] -l [PORT] -c -b [BAUD] -p X -n [NODE]","QMXFER.COM -r -f [FILE] -l [PORT] -c -b [BAUD] -p X -n [NODE]"
"C) Crc-xmodem_______(Internal)
",0,IC,8,,,128,,0.78,,,,
"1) Crc-xmodem_______(Qmxfer)
",0,S,8,,,128,,0.78,,,"C:QMXFER.COM -s -f [FILE] -l [PORT] -c -b [BAUD] -p C -n [NODE]","QMXFER.COM -r -f [FILE] -l [PORT] -c -b [BAUD] -p C -n [NODE]"
"W) Windowed-xmodem__(Wxmodem)
",0,S,,,,128,,0.78,,,"C:WXMODEM.COM -s -f [FILE] -l [PORT] -c -b [BAUD] -p W -n [NODE]","WXMODEM.COM -r -f [FILE] -l [PORT] -c -b [BAUD] -p W -n [NODE]"
"Y) Ymodem-xmodem1K__(Internal)
",0,IY,8,,,1024,,0.87,,,,
"3) Ymodem-xmodem1K__(Qmxfer)
",0,S,8,,,1024,,0.87,,,"C:QMXFER.COM -s -f [FILE] -l [PORT] -c -b [BAUD] -p Y -n [NODE]","QMXFER.COM -r -f [FILE] -l [PORT] -c -b [BAUD] -p Y -n [NODE]"
"B) Ymodem-batch_____(Dsz)
",0,S,8,,B,1024,,0.90,,1=E,"C:dsz.com port [PORT#] speed [BAUD] sb -k [FILE]","dsz.com port [PORT#] speed [BAUD] rb [FILE]"
"G) Ymodem-g_________(Qmxfer)
",0,S,8,R,,1024,,0.90,,,"C:QMXFER.COM -s -f [FILE] -l [PORT] -c -b [BAUD] -p G -n [NODE]","QMXFER.COM -r -f [FILE] -l [PORT] -c -b [BAUD] -p G -n [NODE]"
"I) Imodem___________(Qmxfer)
",0,S,8,R,,128,,0.90,,,"C:QMXFER.COM -s -f [FILE] -l [PORT] -c -b [BAUD] -p I -n [NODE]","QMXFER.COM -r -f [FILE] -l [PORT] -c -b [BAUD] -p I -n [NODE]"
"J) Jmodem___________(Jmodem)
",0,S,8,,,8192,F,0.90,,1=E,"C:\RBBS\JMODEM.COM S[PORT#] [FILE]","C:\RBBS\JMODEM.COM R[PORT#] [FILE]"
"P) Jmodem-batch_____(SuperK)
",0,S,8,,B,0,,0.87,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] Sjb f [FILE]","SUPERK.COM p[PORT#] s[BAUD] n[NODE] r Rjb f [FILE]"
"K) Kermit___________(PCkermit)
",0,S,,,,128,F,0.78,,,"C:PCKERMIT.EXE -s [FILE] -l [PORT] -c -b [BAUD] -p [PARITY] -m 31","PCKERMIT.EXE -r -a [FILE] -l [PORT] -c -b [BAUD] -p [PARITY] -m 31"
"S) Super8k-batch____(SuperK)
",0,S,8,,B,0,,0.92,,4=F,"SUPERK.COM p[PORT#] s[BAUD] n[NODE] Ssb f [FILE]","SUPERK.COM p[PORT] s[BAUD] n[NODE] r Rsb f [FILE]"
"Z) Zmodem-batch_____(Dsz)
",0,S,8,,B,1024,,0.95,,1=E,"C:dsz.com port [PORT#] speed [BAUD] sz -mZ [FILE]","dsz.com port [PORT#] speed [BAUD] rz -mZ [FILE]"
"R) Zmodem-recover___(Dsz)
",0,S,8,,B,1024,,0.95,,1=E,"C:\RBBS\dsz.com port [PORT#] speed [BAUD] sz -rmZ [FILE]","C:\RBBS\dsz.com port [PORT#] speed [BAUD] rz -rmZ [FILE]"
"M) Bimodem-batch____(ErikLabs)
",0,D,8,,B,2030,,0.95,,4=E=A,"BIMUP.BAT [BAUD] [NODE] [FILE] [PROTO]","BIMDN.BAT [BAUD] [NODE] [FILE] [PROTO]"
"A) Ascii____________(Internal)
",0,IA,,,,,,0.92,,,,
"N) None_____________(Cancel)

Select Protocol",4,IN,,,,,,,,,,
